//1971 BRM engine V.Moyet www.CREW.m4driving.sm
RPMTorque=( 0.0, -17.6, -10.0)
RPMTorque=( 250.0, -25.3, 39.4)
RPMTorque=( 500.0, -30.5, 85.8)
RPMTorque=( 1000.0, -34.6, 130.5)
RPMTorque=( 1500.0, -39.4, 166.3)
RPMTorque=( 2000.0, -44.3, 199.6)
RPMTorque=( 2500.0, -49.2, 235.4)
RPMTorque=( 3000.0, -56.5, 270.3)
RPMTorque=( 3500.0, -59.8, 297.2)
RPMTorque=( 4000.0, -64.6, 320.7)
RPMTorque=( 4250.0, -69.5, 338.6)
RPMTorque=( 4500.0, -72.0, 350.8)
RPMTorque=( 4750.0, -76.8, 361.4)
RPMTorque=( 5000.0, -79.3, 366.3)
RPMTorque=( 5250.0, -81.7, 368.8)
RPMTorque=( 5500.0, -81.7, 371.1)
RPMTorque=( 5750.0, -81.7, 372.1)
RPMTorque=( 6000.0, -82.5, 373.2)
RPMTorque=( 6250.0, -84.1, 375.3)
RPMTorque=( 6500.0, -87.3, 375.3)
RPMTorque=( 6750.0, -89.0, 377.5)
RPMTorque=( 7000.0, -89.0, 378.6)
RPMTorque=( 7500.0, -87.3, 374.3)
RPMTorque=( 8000.0, -88.1, 366.7)
RPMTorque=( 8500.0, -89.0, 354.7)
RPMTorque=( 9000.0, -89.0, 338.5)
RPMTorque=( 9500.0, -90.8, 315.7)
RPMTorque=( 10000.0, -93.1, 285.4)
RPMTorque=( 10500.0, -96.3, 258.3)
RPMTorque=( 11000.0, -98.8, 230.5)
RPMTorque=( 11500.0, -101.2, 200.0)
RPMTorque=( 12000.0, -103.7, 178.7)
RPMTorque=( 12500.0, -106.1, 148.2)
FuelConsumption=3.750e-5           // affected by throttle position and engine speed
FuelEstimate=1.000                 // fudge factor for differences between vehicle types (used for lap estimates and AI pit scheduling)
EngineInertia=0.050                // rotational inertia of engine components
IdleThrottle=0.4                   // throttle multiplier to help maintain idle speed
IdleRPMLogic=(1200.0, 1600.0)       // attempt to maintain idle speed between these RPMs
LaunchEfficiency=0.0               // efficiency (0.0-1.0) of launch control, or 0.0 if N/A
LaunchRPMLogic=(7500.0, 9000.0)    // holds RPM in this range before launch (used for AI even if launch control is N/A!)
RevLimitRange=(10500.0,0.0, 00)
RevLimitSetting=0    
RevLimitLogic=50.0                 // RPM range around current setting where rev limiter operates
EngineMapRange=(0, 1, 5)            // 0 = most driveable, max = most power (low gears only) 
EngineMapSetting=2   
EngineBrakingMapRange=(0.0, 0.000133, 6) // input throttle is ranged from minimum to 100%, with the minimum = setting * step * RPM,
EngineBrakingMapSetting=2                // the default is 2 * 0.000125 * 16000 RPM = 4% applied throttle at zero input throttle
OptimumOilTemp=105.0                // degrees Celsius at which engine operates optimally
CombustionHeat=50.0                 // degrees Celsius added per liter of fuel burned
EngineSpeedHeat=2.700e-003        // heat added linearly with engine speed
OilMinimumCooling=9.100e-004         // heat dissipated without radiator
OilWaterHeatTransfer=(7.500e-003,9.800e-005)    // heat transfer from oil to water (base, w/ 
WaterMinimumCooling=2.300e-003      // heat dissipated without radiator
RadiatorCooling=(1.600e-003, 3.100e-004)        // cooling rate with velocity (base, per 
LifetimeEngineRPM=(10250.0,90.0)   // (base engine speed for lifetime, range where lifetime 
LifetimeOilTemp=(116.0,0.40)       // (base oil temp for lifetime, range where lifetime is 
LifetimeAvg=7500                   // average lifetime in seconds
LifetimeVar=3026                    // lifetime random variance
EngineEmission=(0.0, 0.50, -0.500)     // where flames and smoke are emitted (relative to ref 
OnboardStarter=1                    // whether vehicle restarts when stalled
StarterTiming=(1.2, 0.4, 1.5)       // average and variable cranking time, then time to blend
SpeedLimiter=0  