////////////////////////////////////////////////////////////////
//
//  ****************************************    
//   246GT SUSPENSION BY philcout 01/09
//  ****************************************
//  	  - rFactor version - 
//
// - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -
//  Modification, re-use or re-release of these sound
//  files are expressly forbidden
//  without the author's expressed permission!
// - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -
//
////////////////////////////////////////////////////////////////


[BODY]
name=body mass=(0.0) inertia=(0.0,0.0,0.0)
pos=(0.0,0.0,0.0) ori=(0.0,0.0,0.0)

// Front spindles
[BODY]
name=fl_spindle mass=(14.5) inertia=(0.0275,0.0260,0.0245)
pos=(0.72,0.0,-1.075) ori=(0.0,0.0,0.0)

[BODY]
name=fr_spindle mass=(14.5) inertia=(0.0275,0.0260,0.0245)
pos=(-0.72,0.0,-1.075) ori=(0.0,0.0,0.0)

// Front wheels
[BODY]
name=fl_wheel mass=(22.0) inertia=(0.970,0.724,0.724)
pos=(0.72,0.0,-1.075) ori=(0.0,0.0,0.0)

[BODY]
name=fr_wheel mass=(22.0) inertia=(0.970,0.724,0.724)
pos=(-0.72,0.0,-1.075) ori=(0.0,0.0,0.0)

// Rear spindles
[BODY]
name=rl_spindle mass=(14.0) inertia=(0.0275,0.0260,0.0245)
pos=(0.75,0.0,1.35) ori=(0.0,0.0,0.0)

[BODY]
name=rr_spindle mass=(14.0) inertia=(0.0275,0.0260,0.0245)
pos=(-0.75,0.0,1.35) ori=(0.0,0.0,0.0)

// Rear wheels (includes half of rear-axle)
[BODY]
name=rl_wheel mass=(25.0) inertia=(1.190,0.724,0.724)
pos=(0.75,0.0,1.35) ori=(0.0,0.0,0.0)

[BODY]
name=rr_wheel mass=(25.0) inertia=(1.190,0.724,0.724)
pos=(-0.75,0.0,1.35) ori=(0.0,0.0,0.0)

// Fuel in tank is not rigidly attached - it is attached with springs and
// dampers to simulate movement.  Properties are defined in the HDV file.
[BODY]
name=fuel_tank mass=(1.0) inertia=(1.0,1.0,1.0)
pos=(0.0,0.0,0.0) ori=(0.0,0.0,0.0)

[BODY]
name=driver_head mass=(5.0) inertia=(0.02,0.02,0.02)
pos=(0.0,0.0,0.0) ori=(0.0,0.0,0.0)

// Front wheel and spindle connections
[JOINT&HINGE]
posbody=fl_wheel negbody=fl_spindle pos=fl_wheel axis=(-1.000,0.0,0.0)

[JOINT&HINGE]
posbody=fr_wheel negbody=fr_spindle pos=fr_wheel axis=(1.000,0.0,0.0)


// Front left suspension (2 A-arms + 1 steering arm = 5 links)
[BAR] // forward upper arm
name=fl_fore_upper posbody=body negbody=fl_spindle pos=(0.410,0.188,-1.05) neg=(0.613,0.228,-1.050)

[BAR] // rearward upper arm
posbody=body negbody=fl_spindle pos=(0.410,0.188,-0.85) neg=(0.613,0.228,-1.050)

[BAR] // forward lower arm
posbody=body negbody=fl_spindle pos=(0.370,-0.160,-1.05) neg=(0.698,-0.160,-1.05)

[BAR] // rearward lower arm
name=fl_fore_lower posbody=body negbody=fl_spindle pos=(0.370,-0.160,-0.80) neg=(0.698,-0.160,-1.05)

[BAR] // steering arm (must be named for identification)
name=fl_steering posbody=body negbody=fl_spindle pos=(0.392,-0.104,-1.215) neg=(0.650,-0.088,-1.222)


// Front right suspension (2 A-arms + 1 steering arm = 5 links)
[BAR] // forward upper arm (used in steering lock calculation)
name=fr_fore_upper posbody=body negbody=fr_spindle pos=(-0.410,0.188,-1.05) neg=(-0.613,0.228,-1.050)

[BAR] // rearward upper arm
posbody=body negbody=fr_spindle pos=(-0.410,0.188,-0.85) neg=(-0.613,0.228,-1.050)

[BAR] // forward lower arm
name=fr_fore_lower posbody=body negbody=fr_spindle pos=(-0.370,-0.160,-1.05) neg=(-0.698,-0.160,-1.05)

[BAR] // rearward lower arm
posbody=body negbody=fr_spindle pos=(-0.370,-0.160,-0.80) neg=(-0.698,-0.160,-1.05)

[BAR] // steering arm (must be named for identification)
name=fr_steering posbody=body negbody=fr_spindle pos=(-0.392,-0.104,-1.215) neg=(-0.650,-0.088,-1.222)


// Rear left suspension (2 A-arms + 1 straight link = 5 links)
[BAR] // forward upper arm
posbody=body negbody=rl_spindle pos=(0.600,0.00,0.865) neg=(0.600,0.100,1.350)

[BAR] // rearward upper arm
posbody=body negbody=rl_spindle pos=(0.150,0.060,1.350) neg=(0.600,0.100,1.350)

[BAR] // forward lower arm
posbody=body negbody=rl_spindle pos=(0.600,-0.00,0.865) neg=(0.600,-0.100,1.350)

[BAR] // rearward lower arm
posbody=body negbody=rl_spindle pos=(0.150,-0.075,1.350) neg=(0.600,-0.100,1.350)

[BAR] // straight link
posbody=body negbody=rl_spindle pos=(0.150,-0.00,1.350) neg=(0.600,0.0,1.450)


// Rear right suspension (2 A-arms + 1 straight link = 5 links)
[BAR] // forward upper arm
posbody=body negbody=rr_spindle pos=(-0.600,0.00,0.865) neg=(-0.600,0.100,1.350)

[BAR] // rearward upper arm
posbody=body negbody=rr_spindle pos=(-0.150,0.060,1.350) neg=(-0.600,0.100,1.350)

[BAR] // forward lower arm
posbody=body negbody=rr_spindle pos=(-0.600,-0.00,0.865) neg=(-0.600,-0.100,1.350)

[BAR] // rearward lower arm
posbody=body negbody=rr_spindle pos=(-0.150,-0.075,1.350) neg=(-0.600,-0.100,1.350)

[BAR] // straight link
posbody=body negbody=rr_spindle pos=(-0.150,-0.00,1.350) neg=(-0.600,0.0,1.450)

// Rear spindle and wheel connections
[JOINT&HINGE]
posbody=rl_wheel negbody=rl_spindle pos=rl_wheel axis=(-1.00,0.0,0.0)

[JOINT&HINGE]
posbody=rr_wheel negbody=rr_spindle pos=rr_wheel axis=(1.00,0.0,0.0)
