// Engine data generated by PhysicsEditor
RPMTorque=( 0.0, -5.5, -10.0)
RPMTorque=( 250.0, -7.7, 12.0)
RPMTorque=( 500.0, -10.3, 23.9)
RPMTorque=( 750.0, -12.9, 35.7)
RPMTorque=( 1000.0, -15.6, 47.5)
RPMTorque=( 1250.0, -18.5, 59.0)
RPMTorque=( 1500.0, -21.4, 70.3)
RPMTorque=( 1750.0, -24.5, 81.4)
RPMTorque=( 2000.0, -27.6, 92.1)
RPMTorque=( 2250.0, -30.8, 102.4)
RPMTorque=( 2500.0, -34.1, 112.3)
RPMTorque=( 2750.0, -37.1, 121.8)
RPMTorque=( 3000.0, -40.8, 130.7)
RPMTorque=( 3250.0, -44.2, 139.1)
RPMTorque=( 3500.0, -47.6, 150.3)
RPMTorque=( 3750.0, -51, 159.4)
RPMTorque=( 4000.0, -54.4, 169.7)
RPMTorque=( 4250.0, -57.9, 181.6)
RPMTorque=( 4500.0, -61.2, 192.5)
RPMTorque=( 4750.0, -64.6, 204.4)
RPMTorque=( 5000.0, -67.9, 211.8)
RPMTorque=( 5250.0, -71.1, 221.5)
RPMTorque=( 5500.0, -74.3, 230.0)
RPMTorque=( 5750.0, -77.4, 231.8)
RPMTorque=( 6000.0, -80.4, 231.2)
RPMTorque=( 6250.0, -83.3, 229.5)
RPMTorque=( 6500.0, -86.1, 227.2)
RPMTorque=( 6750.0, -88.8, 224.9)
RPMTorque=( 7000.0, -91.3, 220.4)
RPMTorque=( 7250.0, -93.7, 215.8)
RPMTorque=( 7500.0, -96, 211.3)
RPMTorque=( 7750.0, -98, 205.0)
RPMTorque=( 8000.0, -99.9, 199.9)
RPMTorque=( 8250.0, -101.64, 191.3)
RPMTorque=( 8500.0, -103.1, 175.9)
RPMTorque=( 8750.0, -104.4, 151.5)
RPMTorque=( 9000.0, -105.5, 114.4)
RPMTorque=( 9250.0, -106.4, 67.7)
RPMTorque=( 9500.0, -107, 16.5)
RPMTorque=( 9750.0, -107.3, -7.7)
RPMTorque=( 10000.0, -107.4, -33.9)
FuelConsumption=4.400e-005          // affected by throttle position and engine speed
FuelEstimate=1.020                  // fudge factor for differences between vehicle types (used for lap estimates and AI pit scheduling)
EngineInertia=0.1725
IdleThrottle=1.00
IdleRPMLogic=(1687.50, 1887.50)
LaunchEfficiency=0.000              // efficiency (0.0-1.0) of launch control, or 0.0 if N/A
LaunchRPMLogic=(3000.0, 4000.0)     // holds RPM in this range before launch (used for AI even if launch control is N/A!)
RevLimitRange=(8000.0, 100.0, 1) origine
RevLimitSetting=0
RevLimitLogic=150.0                 // RPM range around current setting where rev limiter operates
EngineMapRange=(0, 1, 1)            // 0 = most driveable, max = most power (low gears only) (unimplemented)
EngineMapSetting=0
EngineBrakingMapRange=(0.0, 0.001, 1) // input throttle is ranged from minimum to 100%, with the minimum = setting * step * RPM,
EngineBrakingMapSetting=0             // i.e. if you want 10% throttle at 6000 RPM, set the middle number to 10/6000 = 0.00167
OptimumOilTemp=100.5                // degrees Celsius at which engine operates optimally
CombustionHeat=41.0                 // degrees Celsius added per liter of fuel burned
EngineSpeedHeat=8.000e-004          // heat added linearly with engine speed
OilMinimumCooling=7.200e-003        // heat dissipated without oil/water transfer
OilWaterHeatTransfer=(3.962e-001,7.925e-005)  // heat transfer from oil to water (base, w/ engine speed)
WaterMinimumCooling=3.562e-003      // base heat dissipated without velocity
RadiatorCooling=(2.292e-004, 4.510e-006)      // cooling rate with velocity (base, per setting)
LifetimeEngineRPM=(7500.0,180.0)   // (base engine speed for lifetime, range where lifetime is halved)
LifetimeOilTemp=(108.0,2.50)        // (base oil temp for lifetime, range where lifetime is halved)
LifetimeAvg=30000                   // average lifetime in seconds
LifetimeVar=5500                    // lifetime random variance
EngineEmission=(0.20, 0.60, -2.5)   // where flames and smoke are emitted (relative to ref frame at rear axle)
EngineSound=(0.20, 0.60, -2.5)      // where engine sound is emitted (relative to ref frame at rear axle)
SpeedLimiter=0                      // whether there is a pitlane speed limiter
OnboardStarter=1                    // whether vehicle restarts when stalled
StarterTiming=(1.5, 0.0, 0.0)       // average and variable cranking time, then blend with starting sound